### Product information 40/2016

**FORD Focus III RS**

Focus III RS, type DYB, from 2016 - 2.3l 257 kW (YVDA)

REMUS Cat-Back system

* 100% stainless steel
* Powerful sound
* Performance and torque increase
* EEC homologation

- 6,6 kg

+ 11,5 Nm





**0026 80S**

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **FORD Focus III RS, type DYB, 2016=>** 2.3l 257 kW (YVDA) | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **206516 1500** | **Cat-Back system** L/R (without tail pipes)  With integrated valve with EEC homologation.  Original tube Ø 70 mm REMUS tube Ø 76 mm | **1.090,--** |
| **0026 80S** | Stainless steel tail pipe set 2 tail pipes Ø 115 mm angled, chromed, with adjustable spherical clamp connection | **180,--** |
|  | | |
| **INFOBOX:**   * **Cat-Back system:** **206516 1500 +** **tail pipe set!** No cutting of the original exhaust system required! * **C:\Users\benjamin.druck\Desktop\ki\REMUS Produktinformation 40-2016 Ford Focus RS\LD_Ford_Focus_III_RS_o.jpg206516 1500 +** **tail pipe set** only fits as a complete system! * The activation of the valve is carried out using the original actuator via the vehicle onboard electronics. | | |

**REMUS Powerizer**

**More power, more economy and more fun!**

The electronics of the REMUS Powerizer enhances in real time  
 the engine management parameter. The engine mapping  
 is optimized in excess of 1000 times per second and ensures for a  
 considerable and noticeable power increase. The engine safety parameters and management remains totally original to ensure that individual engine components are not overstrained. Furthermore, the original mapping software remains totally untouched.

Due to the Plug & Play concept, the REMUS Powerizer is simple to install and can be easily removed or decommissioned using the supplied blind connector. Due to the torque increase, the engine has more power at lower RPM which leads to a reduction in fuel consumption. The power increase of the engine can be adjusted according to different driving styles by means of a „maximum power setting“, „eco fuel saving mode“ or a combination of both. The REMUS Powerizer is available for over 3000 petrol and diesel powered cars.





* Up to 25% more power
* Up to 20% more torque
* Easy installation and removal (Plug & Play)
* Up to 1l/100 km fuel saving
* 3 preset programs (RACE/SPORT/ECO) with individual power adjustment

**REMUS Responder**

**Improved throttle response, more dynamic!**

Der REMUS ResponderThe REMUS Responder improves throttle response by means  
 of modifying the accelerator pedal output signal.  
  
 No more throttle delay and reduced lag during automatic shifting makes driving  
 with the REMUS Responder more fun. The Responder attaches between the   
OEM pedal sensor and the OEM connector, ready to use in seconds due to plug & play technology.

Sophisticated adjustable programming profiles can lead to improved fuel consumption and

more efficiency. The 4 individual user selectable and adjustable performance settings

allow drivers to select according to their own preferences. The REMUS Responder totally eliminates the delay in modern electronic accelerator pedals!



* Improved throttle response, reduced lag during gear changes
* Quicker reaction times, more dynamic without changing engine parameters
* 4 individual user selectable and adjustable performance settings
* Vehicle specific programming using OEM quality connectors
* Simple plug & play installation and easily removed without leaving traces

