

Product information 18/2018

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **BMW M2 Competition F87N Coupe, 09/2018=>**  3.0l 302 kW (S55B30, with GPF, EURO 6d-TEMP) | | |
| **INFOBOX:**   * **RACING axle-back-system L/R:** 088318 1500 (No EC type approval)+ tail pipe set! The original exhaust will need to be cut! No rear skirt modifications required! * The use of racing products and products which do not have EC approval is generally not permitted on public roads. * When installing REMUS axle-back and cat-back or catalyst delete tubes on vehicles which are used for closed road driving, it is advisable to tune the ECU for a maximum gain in performance and to ensure that the CEL does not come on. | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **088318 1500** | |  | | --- | | RACING axle-back sport exhaust system, stainless steel,  with integrated valves  Original tube Ø 65 mm - REMUS tube Ø 70 mm  No EC type approval  The activation of the valves is carried out using the original actuators  via the vehicle onboard electronics. | | **1.790,--** |
| **Choose from following tail pipe package:** | | |
| **0046 70SG** | Stainless steel tail pipe set 4 tail pipes Ø 102 mm angled, straight cut, chromed, with adjustable spherical clamp connection | **296,--** |
| **0046 70S** | Stainless steel tail pipe set 4 tail pipes Ø 102 mm angled, rolled edge, chromed, with adjustable spherical clamp connection | **340,--** |
| **0046 70CS** | Carbon tail pipe set 4 tail pipes Ø 102 mm angled, Titanium internals, with adjustable spherical clamp connection | **840,--** |
| **0046 98C** | Stainless steel tail pipe set 4 tail pipes Ø 98 mm Street Race, straight, carbon insert, with adjustable spherical clamp connection | **444,--** |
| **0046 98CB** | Stainless steel tail pipe set 4 tail pipes Ø 98 mm Street Race Black Chrome, straight, carbon insert, with adjustable spherical clamp connection | **492,--** |
|  | | |