

Product information 21/2019

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **VW Golf VII GTI Performance Facelift, type AU, 11/2018=>**  2.0l TSI 180 kW (DKTB, with GPF) | | |
| **INFOBOX:**   * **Axle-back-system dual L/R, for original rear skirt:** 955213 0000 + 796117 1500 or 956017 1600 (No EC type approval) + tail pipe set! The original exhaust must be cut! No rear skirt modifications required! * **GPF-back-system dual L/R, for original rear skirt:** 796118 0300 or 955213 1000 (No EC type approval) + 955213 0000 + 796117 1500 or 956017 1600 (No EC type approval) + tail pipe set! No vehicle modifications required! * The use of racing products and products which do not have EC approval is generally not permitted on public roads. * When installing REMUS axle-back and cat-back or catalyst delete tubes on vehicles which are used for closed road driving, it is advisable to tune the ECU for a maximum gain in performance and to ensure that the CEL does not come on. | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **955213 1000** | Non-resonated RACING GPF-back section, replaces original front silencer, can only be installed in combination with the REMUS sport exhaust,  Original tube Ø 65 mm - REMUS tube Ø 70 mm  No EC type approval | **185,--** |
| **796118 0300** | Resonated GPF-back front section, can only be installed in combination with the REMUS sport exhaust or non resonated L/R Racing system, incl. EC type approval  Original tube Ø 65 mm - REMUS tube Ø 70 mm | **346,--** |
| **955213 0000** | Connection tube for mounting the L/R sport exhaust or the non-resonated L/R RACING systems | **105,--** |
| **796117 1500** | Sport exhaust centered dual for L/R system (without tail pipes, without connecting tube),  suitable for the original rear skirt, incl. EC type approval  Original tube Ø 65 mm - REMUS tube Ø 70 mm | **369,--** |
| **956017 1600** | Non resonated dual L/R RACING system (without tail pipes, without connecting tube), suitable for the original rear skirt  Original tube Ø 65 mm - REMUS tube Ø 70 mm  No EC type approval | **260,--** |
| **Choose from following tail pipe package:** | | |
| **0026 70SG** | Stainless steel tail pipe set 2 tail pipes Ø 102 mm angled, straight cut, chromed, with adjustable spherical clamp connection | **154,00** |
| **0026 70S** | Stainless steel tail pipe set 2 tail pipes Ø 102 mm angled, rolled edge, chromed, with adjustable spherical clamp connection | **178,00** |
| **0026 70CS** | Carbon tail pipe set 2 tail pipes Ø 102 mm angled, Titanium internals, with adjustable spherical clamp connection | **438,00** |
| **0026 98C** | Stainless steel tail pipe set 2 tail pipes Ø 98 mm Street Race, straight, carbon insert, with adjustable spherical clamp connection | **232,00** |
| **0026 98CB** | Stainless steel tail pipe set 2 tail pipes Ø 98 mm Street Race Black Chrome, straight, carbon insert, with adjustable spherical clamp connection | **256,00** |

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **VW Golf VII GTI Performance Facelift, type AU, 11/2018=>**  2.0l TSI 180 kW (DKTB, with GPF) | | |
| **INFOBOX:**   * **Axle-back-system quad L/R:** 955213 0000 + 957117 1500 + tail pipe set! The original exhaust must be cut! Can only be installed in combination using the original diffusor of the VW Golf VII R Facelift, VW part no. 5G6 807 568 AA. * **GPF-back-system quad L/R:** 796118 0300 or 955213 1000 (No EC type approval) + 955213 0000 + 957117 1500 + tail pipe set! No cutting of the original exhaust system required! Can only be installed in combination using the original diffusor of the VW Golf VII R Facelift, VW part no. 5G6 807 568 AA. * The use of racing products and products which do not have EC approval is generally not permitted on public roads. * When installing REMUS axle-back and cat-back or catalyst delete tubes on vehicles which are used for closed road driving, it is advisable to tune the ECU for a maximum gain in performance and to ensure that the CEL does not come on. | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **955213 1000** | Non-resonated RACING GPF-back section, replaces original front silencer, can only be installed in combination with the REMUS sport exhaust,  Original tube Ø 65 mm - REMUS tube Ø 70 mm  No EC type approval | **185,--** |
| **796118 0300** | Resonated GPF-back front section, can only be installed in combination with the REMUS sport exhaust or non resonated L/R Racing system, incl. EC type approval  Original tube Ø 65 mm - REMUS tube Ø 70 mm | **346,--** |
| **955213 0000** | Connection tube for mounting the L/R sport exhaust or the non-resonated L/R RACING systems | **105,--** |
| **957117 1500** | Sport exhaust quad L/R system ( without tail pipes, without connecting tube), incl. EC type approval  Original tube Ø 65 mm - REMUS tube Ø 70 mm  Can only be installed in combination using the original diffusor of the VW Golf VII R Facelift, VW part no. 5G6 807 568 AA. | **699,--** |
| **Choose from following tail pipe package:** | | |
| **0046 70SG** | Stainless steel tail pipe set 4 tail pipes Ø 102 mm angled, straight cut, chromed, with adjustable spherical clamp connection | **308,00** |
| **0046 70S** | Stainless steel tail pipe set 4 tail pipes Ø 102 mm angled, rolled edge, chromed, with adjustable spherical clamp connection | **356,00** |
| **0046 70CS** | Carbon tail pipe set 4 tail pipes Ø 102 mm angled, Titanium internals, with adjustable spherical clamp connection | **876,00** |
| **0046 98C** | Stainless steel tail pipe set 4 tail pipes Ø 98 mm Street Race, straight, carbon insert, with adjustable spherical clamp connection | **464,00** |
| **0046 98CB** | Stainless steel tail pipe set 4 tail pipes Ø 98 mm Street Race Black Chrome, straight, carbon insert, with adjustable spherical clamp connection | **492,00** |