

Product information 27/2019

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **MINI John Cooper Works “JCW” F57 Cabrio, type WJ91 (3 door), 01/2019=>**  2.0l Turbo 170 kW (with GPF) | | |
| **INFOBOX:**   * **Axle-back-system centered:** 753019 5500 + tail pipe set! The original exhaust must be cut! No rear skirt modifications required! * **RACING-axle-back-system centered:** 752719 5500 (No EC type approval) + tail pipe set + optional STE 0003BT (No EC type approval)! The original exhaust must be cut! No rear skirt modifications required! * The use of racing products and products which do not have EC approval is generally not permitted on public roads. * When installing REMUS axle-back and cat-back or catalyst delete tubes on vehicles which are used for closed road driving, it is advisable to tune the ECU for a maximum gain in performance and to ensure that the CEL does not come on. | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **753019 5500** | Sport exhaust centered (without tail pipes)  incl. EC type approval  Original tube Ø 60 mm - REMUS tube Ø 70 mm | **495,--** |
| **752719 5500** | RACING sport exhaust centered (without tail pipes)  with integrated valve  No EC type approval  Original tube Ø 60 mm - REMUS tube Ø 70 mm  It is not permissible to activate the valve on public roads as per the EU transport authority.  The activation of the valve can be carried out using the seperate available REMUS sound controller. The sound controller and electrical actuator allows the valve to be operated in 4 different positions. | **590,--** |
| **Optional (only for RACING sport exhaust system 752719 5500):**  **REMUS Sound Controller (APP-compatible)** | | |
| **STE 0003BT** | The REMUS Sound Controller (APP-compatible) consisting of the electronic module, the OBDII plug, the remote control button as well as the electrical actuator including the cables.  No EC type approval | **499,00** |
| **Choose from following tail pipe package:** | | |
| **0026 70SG** | Stainless steel tail pipe set 2 tail pipes Ø 102 mm angled, straight cut, chromed, with adjustable spherical clamp connection | **154,00** |
| **0026 70S** | Stainless steel tail pipe set 2 tail pipes Ø 102 mm angled, rolled edge, chromed, with adjustable spherical clamp connection | **178,00** |
| **0026 70CS** | Carbon tail pipe set 2 tail pipes Ø 102 mm angled, Titanium internals, with adjustable spherical clamp connection | **438,00** |
| **0026 98C** | Stainless steel tail pipe set 2 tail pipes Ø 98 mm Street Race, straight, carbon insert, with adjustable spherical clamp connection | **232,00** |
| **0026 98CB** | Stainless steel tail pipe set 2 tail pipes Ø 98 mm Street Race Black Chrome, straight, carbon insert, with adjustable spherical clamp connection | **256,00** |
|  | | |