**REMUS product information 06-2015**

**MERCEDES BENZ CLA 45 AMG, C117, 2014=>**

**MERCEDES BENZ A 45 AMG, W176, 2013=>**

Dear **REMUS**-Partner,

We are pleased to inform you that we have completed our next development

**REMUS Cat-back system incl. front section and optional REMUS Sound Controller for the**

**Mercedes Benz CLA 45 AMG, C117, 2014=>**

**Mercedes Benz A 45 AMG, W176, 2013=>**

It would be a pleasure for us to receive your order.

Stay tuned!

Your **REMUS** Team

|  |
| --- |
| **Car and engine specification** |
| **Mercedes Benz CLA 45 AMG, C117, 2014=>****Mercedes Benz A 45 AMG, W176, 2013=>**2.0l 265 kW |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **504013 1500** | Stainless steel Cat-back system, centered including electronic controlled valve and non resonated front section, with homologation | **1.180,--** |
| **choose from following outlet tubes:** |
| **504013 1600** | Stainless steel outlet tubes for **A 45 AMG** incl. installation kit, suitable for the original exhaust outlets | **110,--** |
| **504513 1600** | Stainless steel outlet tubes for **CLA 45 AMG** incl. installation kit, suitable for the original exhaust outlets | **110,--** |
|  |
| **Optional: REMUS Sound Controller** |
| **STE 0002** | Sound Controller consisting of:Electronic module incl. remote control for individual sound in 4 levels, no homologation | **290,--** |
|  |
| **ATTENTION:** * Cat-back system can only be installed using the required outlet tubes!
 |

****



|  |  |  |
| --- | --- | --- |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **B917823** | **REMUS POWERIZER for**MB CLA (C117) (2013-...) 45 AMG 2.0 360 HP 4MATICOriginal: 265 kW / 360 HP / 450 NmTUNED: 298 kW / 405 HP / 518 Nm / Vmax + - kmH | **499,--** |
| **B918426** | **REMUS POWERIZER for**MB Class A (W176) (2012-...) 45 AMG 2.0 360 HP 4MATICOriginal: 265 kW / 360 HP / 450 NmTUNED: 298 kW / 405 HP / 518 Nm / Vmax + 0 kmH | **499,--** |
| **REMUS Powerizer: More power, more economy and more fun.*** Up to 25 % more power
* Up to 20 % more torque
* Up to 1l/100 km fuel saving
* Fully adjustable power increase
* Simple DIY installation (Plug & Play)

REMUS POWERIZER: The performance figures represent the maximum achievable values. The actual performance output depends on the original tolerances of each engine. REMUS delivers the POWERIZER with the best possible setting for your vehicle type. You can adjust the performance according to your requirements as per the POWERIZER instructions**Legal references***1. Completion and registration of chip tuning in the car documents*Due to chip tuning, the operating license of the vehicle will terminate if the installation and registration of the POWERIZER is not carried out or immediately reported to an official approved testing facility. Please consider that driving a vehicle without the required operating license will cause legal penalties.*2. Vehicle insurance must be informed upon installing a POWERIZER*The installation of the POWERIZER can have influence on the insurance policy of your vehicle. You must inform the insurance company if you install a POWERIZER in your vehicle.*3. Effect of chip tuning on warranty and guarantee claims*a) When installing a POWERIZER, you will lose all guarantee claims regarding the engine against the vehicle manufacturer.b) Installing a POWERIZER, can have influence on warranty claims against the seller of the vehicle.c) REMUS excludes any claims regarding compensation for damages on the engine and drivetrain..c) REMUS schließt Ansprüche des Kunden auf Schadenersatz für etwaige Schäden an Motor und Antriebsstrang aus. |





|  |  |  |
| --- | --- | --- |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **R903704** | **REMUS Responder**

|  |
| --- |
| Mercedes A-Klasse (W176) (2012-...) A 180 1595 cm³ 90 kW |
| Mercedes A-Klasse (W176) (2012-...) A 180 CDI 1461 cm³ 80 kW |
| Mercedes A-Klasse (W176) (2012-...) A 180 CDI 1796 cm³ 80 kW |
| Mercedes A-Klasse (W176) (2012-...) A 200 1595 cm³ 115 kW |
| Mercedes A-Klasse (W176) (2012-...) A 200 CDI 1796 cm³ 100 kW |
| Mercedes A-Klasse (W176) (2012-...) A 220 CDI 2143 cm³ 125 kW |
| Mercedes A-Klasse (W176) (2012-...) A 250 1991 cm³ 155 kW |
| Mercedes A-Klasse (W176) (2012-...) A 45 AMG 1991 cm³ 265 kW |
| Mercedes A-Klasse (W176) (2012-...) A 180 1595 cm³ 90 kW |
| Mercedes A-Klasse (W176) (2012-...) A 180 CDI 1461 cm³ 80 kW

|  |
| --- |
| Mercedes CLA-Klasse (C117)(2013-...) 180 BlueEFFICIENCY 1595 cm³ 90 kW |
| Mercedes CLA-Klasse (C117)(2013-...) CLA 180 1595 cm³ 115 kW |
| Mercedes CLA-Klasse (C117)(2013-...) CLA 200 1595 cm³ 115 kW |
| Mercedes CLA-Klasse (C117)(2013-...) CLA 200 CDI 1796 cm³ 100 kW |
| Mercedes CLA-Klasse (C117)(2013-...) CLA 220 CDI 2143 cm³ 125 kW |
| Mercedes CLA-Klasse (C117)(2013-...) CLA 250 1991 cm³ 155 kW |
| Mercedes CLA-Klasse (C117)(2013-...) CLA 45 AMG 1991 cm³ 265 kW |

 |

 | **167,--** |
| **REMUS RESPONDER:****Improved throttle response, more dynamic!**The REMUS Responder improves throttle response by means of modifying the accelerator pedal output signal. No more throttle delay and reduced lag during automatic shifting makes driving with the REMUS Responder more fun. The Responder attaches between the OEM pedal sensor and the OEM connector, ready to use in seconds due to plug & play technology. Sophisticated adjustable programming profiles can lead to improved fuel consumption and more efficiency. The 4 individual user selectable and adjustable performance settings allow drivers to select according to their own preferences. The REMUS Responder totally eliminates the delay in modern electronic accelerator pedals! |

