

Product information 12/2018

\*

\*

**\***

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **BMW M5 F90 Sedan, 12/2017=>**  4.4l V8 441 kW (S63B44Tx) **without GPF** | | |
| **INFOBOX:**   * **RACING axle-back-system L/R:** 089317 0500LR (No EC type approval) + tail pipe set! The original exhaust must be cut! No rear skirt modifications required! Not for Competition models! * **RACING cat-back-system L/R:** 089317 0000 (No EC type approval) + 089317 0500LR (No EC type approval) + tail pipe set! No vehicle modifications required! Not for Competition models! | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **089317 0000** | Non-resonated cat-back front section, can only be installed in combination with the REMUS axle-back sport exhaust system  Original tube Ø 80 mm - REMUS tube Ø 84 mm  No EC type approval | **650,--** |
| **089317 0500LR** | |  | | --- | | Axle-back sport exhaust system, stainless steel, with integrated valves  Original tube Ø 80 mm - REMUS tube Ø 84 mm  No EC type approval  The activation of the valves is carried out using the original actuators  via the vehicle onboard electronics. | | **1.370,--** |
| **Choose from following tail pipe package:** | | |
| **0446 70CS** | Carbon tail pipe set 4 tail pipes Ø 102 mm angled (shorter length 145 mm), Titanium internals, with adjustable spherical clamp connection | **840,--** |
| **0446 70SG** | Stainless steel tail pipe set 4 tail pipes Ø 102 mm angled (shorter length 145 mm), straight cut, chromed, with adjustable spherical clamp connection | **296,--** |
|  | | |