

Product information 20/2019

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **BMW 4er F33 Cabrio, type 3C, 07/2018=>**  440i xDrive 3.0l Turbo 240 kW (B58B30A, with GPF)  **BMW 4er F32 Coupe, type 3C, 07/2018=>**  440i xDrive 3.0l Turbo 240 kW (B58B30A, with GPF)  **BMW 4er F36 Gran Coupe, type 3C, 07/2018=>**  440i xDrive 3.0l Turbo 240 kW (B58B30A, with GPF) | | |
| **INFOBOX:**   * **Axle-back-system L/R:** 084119 1500 + tail pipe set! The original exhaust must be cut! No rear skirt modifications required! * **Suitable only for cars with M sport option!** | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **084119 1500** | Sport exhaust centered for L/R system (without tail pipes),  with 1 integrated valve, incl. EC type approval  Original tube Ø 80 mm - REMUS tube Ø 84 mm  Suitable only for cars with M sport option!  The activation of the valve is carried out using the original actuator via the vehicle onboard electronics. | **810,--** |
| **Choose from following tail pipe package:** | | |
| **0026 55S** | Stainless steel tail pipe set 2 tail pipes Ø 84 mm angled, rolled edge, chromed, with adjustable spherical clamp connection | **168,--** |
| **0026 05** | Stainless steel tail pipe set 2 tail pipes Ø 90 mm straight, rolled edge, chromed, with adjustable spherical clamp connection | **168,--** |
| **0026 83C** | Stainless steel tail pipe set 2 tail pipes Ø 84 mm Street Race, straight, carbon insert, with adjustable spherical clamp connection | **204,--** |
| **0026 83CS** | Stainless steel tail pipe set 2 tail pipes Ø 84 mm Carbon Race, angled, carbon ring, with adjustable spherical clamp connection | **212,--** |
| **0026 83CB** | Stainless steel tail pipe set 2 tail pipes Ø 84 mm Street Race Black Chrome, straight, carbon insert, with adjustable spherical clamp connection | **230,--** |
| **0026 83CTS** | Carbon tail pipe set 2 tail pipes Ø 84 mm angled, Titanium internals, with adjustable spherical clamp connection | **406,--** |
|  | | |