

Product information 26/2019

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **AUDI RS3 sedan 4door Quattro, type 8V, 2019=>**  **AUDI RS3 Sportback Quattro, type 8V, 2019=>**  2.5l Turbo 294 kW (DNW, with GPF) | | |
| **INFOBOX:**   * **GPF-back-system:** 046517 0300 or 047015 0000 (No EC type approval) + 046517 1500 + tail pipe set! No vehicle modifications required! Resonated front or non-resonated front section and sport exhaust L/R with tail pipe set only fits as a complete system! When installing on the Sportback model, the outlet tubes must be shortened by 120 mm! * The use of racing products and products which do not have EC approval is generally not permitted on public roads. * When installing REMUS axle-back and cat-back or catalyst delete tubes on vehicles which are used for closed road driving, it is advisable to tune the ECU for a maximum gain in performance and to ensure that the CEL does not come on. | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **047015 0000** | Non-resonated RACING GPF-back front section, replaces original front silencer  can only be installed together with REMUS sport exhaust  Original tube Ø 70 mm - REMUS tube Ø 76 mm  No EC type approval | **270,--** |
| **046517 0300** | Resonated GPF-back front section, replaces original front silencer,  can only be installed together with REMUS sport exhaust  incl. EC type approval  Original tube Ø 70 mm - REMUS tube Ø 76 mm | **390,--** |
| **046517 1500** | L/R Sport exhaust centered (without tail pipes)  with 2 integrated valves, incl. EC type approval  Original tube Ø 70 mm - REMUS tube Ø 76 mm  Only for mounting on Sportback: shorten the outlet tubes by 120mm!  The supplied actuators activate the valves to factory preset positions via the vehicle onboard electronics. | **1.260,--** |
| **Choose from following tail pipe package:** | | |
| **0046 83C** | Stainless steel tail pipe set 4 tail pipes Ø 84 mm Street Race, straight, carbon insert, with adjustable spherical clamp connection | **408,--** |
| **0046 83CS** | Stainless steel tail pipe set 4 tail pipes Ø 84 mm Carbon Race, angled, carbon ring, with adjustable spherical clamp connection | **424,--** |
| **0046 83CB** | Stainless steel tail pipe set 4 tail pipes Ø 84 mm Street Race Black Chrome, straight, carbon insert, with adjustable spherical clamp connection | **460,--** |
| **0046 83CTS** | Carbon tail pipe set 4 tail pipes Ø 84 mm angled, Titanium internals, with adjustable spherical clamp connection | **812,--** |
| **0046 55S** | Stainless steel tail pipe set 4 tail pipes Ø 84 mm angled, rolled edge, chromed, with adjustable spherical clamp connection | **336,--** |
| **0026 99CSS** | Carbon tail pipe set 2 tail pipes 175x108 mm angled/angled, Titanium internals, with adjustable spherical clamp connection | **810,--** |