

Product information 02/2020

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **BMW X4 M Competition F98 S58, 05/2019=>**  3.0l Turbo 375 kW (S58B30A, with GPF)  **BMW X4 M F98 S58, 05/2019=>**  3.0l Turbo 353 kW (S58B30A, with GPF) | | |
| **INFOBOX:**   * **Axle-back-system L/R:** 086219 6000 + 086219 1500 (No EC type approval for 3.0l Turbo 353 kW) or 086319 1500 (No EC type approval) + tail pipe set! The original exhaust will need to be cut! No rear skirt modifications required! * **RACING cat-back-system L/R:** 086219 1000 (No EC type approval) + 086219 6000 + 086219 1500 (No EC type approval for 3.0l Turbo 353 kW) or 086319 1500 (No EC type approval) + tail pipe set! No cutting modifications required! * The use of racing products and products which do not have EC approval is generally not permitted on public roads. * When installing REMUS axle-back and cat-back or catalyst delete tubes on vehicles which are used for closed road driving, it is advisable to tune the ECU for a maximum gain in performance and to ensure that the CEL does not come on. | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **086219 1000** | Non-resonated RACING Cat-back-section (GPF replacement section)  Original tube Ø 70 mm - REMUS tube Ø 70 mm  No EC type approval | **394,--** |
| **086219 6000** | Set of connection tubes for mounting the L/R sport exhaust | **269,--** |
| **086219 1500** | Sport exhaust, L/R (without tail pipes),  with 2 integrated valves,  incl. EC type approval for Competition 3.0l Turbo 375 kW - No EC type approval for 3.0l Turbo 353 kW!  Original tube Ø 70 mm - REMUS tube Ø 70 mm  The activation of the valves is carried out using the original actuators via the vehicle onboard electronics. | **2.190,--** |
| **086319 1500** | RACING sport exhaust, L/R (without tail pipes),  with 2 integrated valves,  No EC type approval  Original tube Ø 70 mm - REMUS tube Ø 70 mm  The activation of the valves is carried out using the original actuators via the vehicle onboard electronics. | **1.990,--** |
| **Choose from following tail pipe package:** | | |
| **0046 83C** | Stainless steel tail pipe set 4 tail pipes Ø 84 mm Street Race, straight, carbon insert, with adjustable spherical clamp connection | **408,--** |
| **0046 83CS** | Stainless steel tail pipe set 4 tail pipes Ø 84 mm Carbon Race, angled, carbon ring, with adjustable spherical clamp connection | **424,--** |
| **0046 83CB** | Stainless steel tail pipe set 4 tail pipes Ø 84 mm Street Race Black Chrome, straight, carbon insert, with adjustable spherical clamp connection | **460,--** |
| **0046 83CTS** | Carbon tail pipe set 4 tail pipes Ø 84 mm angled, Titanium internals, with adjustable spherical clamp connection | **812,--** |
| **0046 55S** | Stainless steel tail pipe set 4 tail pipes Ø 84 mm angled, rolled edge, chromed, with adjustable spherical clamp connection | **336,--** |
|  | | |